6 cylinder firing orders:  In-line engines, V6 & flat plane
 

Firing order 1-5-3-6-2-4
	6 Cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6

	TDC compression #1
	Set In & Ex
	Set In
	Set Ex
	Set In
	Set Ex
	on overlap

	TDC compression #6
	on overlap
	Set Ex
	Set In
	Set Ex
	Set In
	Set In & Ex


Firing order 1-4-2-6-3-5
	6 Cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6

	TDC compression #1
	Set 1n & Ex
	Set Ex
	Set In
	Set Ex
	Set In
	on overlap-

	TDC compression #6
	on overlap
	Set In
	Set Ex
	Set In
	Set Ex
	Set In & Ex


Firing order 1-6-5-4-3-2
	6 Cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6

	TDC compression #1
	Set 1n & Ex
	Set In
	Set In
	on overlap
	Set ex
	Set Ex

	TDC compression #4
	on overlap
	Set Ex
	Set Ex
	Set In & Ex
	Set In
	Set In


Firing order 1-2-3-4-5-6
	6 Cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6

	TDC compression #1
	Set In & Ex
	Set Ex
	Set Ex
	on overlap
	Set In
	Set In

	TDC compression #4
	on overlap
	Set In
	Set In
	Set In & Ex
	Set Ex
	Set Ex


