4 Cylinder firing orders:  In-line engines & Flat plane
Firing order 1-3-4-2
	4 Cyl Engine
	No.1
	No.2
	No.3
	No.4

	TDC compression #1
	set In & Ex
	Set In
	Set Ex
	on overlap

	TDC compression #4
	on overlap
	Set Ex
	Set In
	Set In & Ex


Firing order 1-2-4-3
	4 Cyl Engine
	No.1
	No.2
	No.3
	No.4

	TDC compression #1
	set In & Ex
	Set Ex
	Set In
	on overlap

	TDC compression #4
	on overlap
	Set In
	Set Ex
	Set In & Ex


 

